**Aurora Lighting – AR-4 Trim Installation**

1. Always properly isolate the fixture from its power source before performing any maintenance.
2. Remove existing lamp and trim.
3. Squeeze the trim clips and firmly push the trim up into the fixture housing to properly seat the trim in the fixture housing.
4. Gently push the insert (baffle or cone) into the trim until it seats properly.
5. Install new Aurora LED retrofit lamp.